Manufacturer | Model | Modulation | Encoding Method | Encoding Type | Compatibility | Verified | Frequency | Buttons | Comments | Front | Back | Inside |
A |  |  |  |  |  |  |  |  |  |  |  |  |
Aprimatic | TR2 TR4 | AM | Rolling Code | HCS301? | Yes | Yes w/ compatible remote | 433 | 2/4 |  |
Avidsen | 104250 | AM | Fixed Code | ? | Yes | Yes w/ compatible remote | 433 | 4 |  |
Avidsen | 104251 | AM | Fixed Code | ? | Yes | Yes | 433 | 4 |  |
Avidsen | 104257 | AM | Fixed Code | ? | Yes | Yes w/ compatible remote | 433 | 4 |  |
Avidsen | 104715 | AM | Fixed Code/ Learning Remote | ? | Yes | Yes | 433 | 4 |  |
B |  |  |  |  |  |  |  |  |  |  |  |  |
Beninca | TO GO T4 WV T4 WK CUPIDO | AM | Rolling Code | HCS301? | Yes | Yes | 433 | 4 |  |
BFT | Mitto | AM | Rolling Code | HCS301 | Yes | Yes | 433 | 2 | Rolling Code emulated in a PIC 12F609 |
C |  |  |  |  |  |  |  |  |  |  |  |  |
Came | TOP432 | AM | Fixed | 12bits | Yes | Yes w/ compatible remote | 433 | 2 | The Came Top432na is two button version of this self-learning remote control series. The four button version Came Top434NA. Came Top432na is made fully compatible with Came 432M, Came 434M, Came 432S, Came 432SA and Came 434MA. Came Top432na is remote control transmitting at 433.92 MHz, the all possible code combinations are as many as 4096 codes. |
Came | TOP434 | AM | Fixed | 12bits | Yes | No | 433 | 4 | The Came Top432na is two button version of this self-learning remote control series. The four button version Came Top434NA. Came Top432na is made fully compatible with Came 432M, Came 434M, Came 432S, Came 432SA and Came 434MA. Came Top432na is remote control transmitting at 433.92 MHz, the all possible code combinations are as many as 4096 codes. |
Cardin | S449 | FM | ? | ? | No | Yes | 433 | 4 |  |
D |  |  |  |  |  |  |  |  |  |  |  |  |
DEA | GENIE MIO TR-2 | AM | Rolling Code | HCS301? | Yes | Yes w/ compatible remote | 433 | 2/4 |  |
Ditec | GOL4 | AM | Variable | 54bits | Yes | Yes w/ compatible remote | 433 | 4 | Ditec GOL4 is a rolling code remote, which has white LED cover color, while GOL4C is a fixed code remote, which has a red LED cover color. |
Ditec | GOL4C | AM | Fixed | 37bits | Yes | Yes | 433 | 4 | Ditec GOL4 is a rolling code remote, which has white LED cover color, while GOL4C is a fixed code remote, which has a red LED cover color. |
Ditec | BILXP2 | AM | Fixed? | 37bits? | Yes | Yes | 433 | 2/4 |  |
Doorhan |  | AM | Rolling Code | HCS301? | Yes | Yes w/ compatible remote | 433 | 4 |  |
E |  |  |  |  |  |  |  |  |  |  |  |  |
Erreka | SOL2R SOL4R ROLLER4 | AM | Rolling Code | HCS301? | Yes | Yes w/ compatible remote | 433 | 4 |  |
Etdoor | ? | AM | ? | ? | Yes | Yes w/ compatible remote | 433 | 2 |  |
F |  |  |  |  |  |  |  |  |  |  |  |  |
FAAC | XT4 433 | AM | Rolling Code | HCS301? | Yes | Yes w/ compatible remote | 433 | 2/4 |  |
Fox |  | AM | Rolling Code | HCS301? | Yes | Yes w/ compatible remote | 433 | 2 |  |
G |  |  |  |  |  |  |  |  |  |  |  |  |
GBD | DOMINO AU1600 | AM | Rolling Code | HCS301? | Yes | Yes w/ compatible remote | 433 | 2 |  |
K |  |  |  |  |  |  |  |  |  |  |  |  |
Key | TXP-42 | AM | Million Code | HT6P20 28bits | Yes | Yes | 433 | 2 |  |
Key | ? | AM | Million Code | eV1527 24bits | Yes | Yes | 433 | 4 |  |
KINGgates | ? | AM | Encrypted |  | Yes | Yes | 433 | 4 |  |
L |  |  |  |  |  |  |  |  |  |  |  |  |
Life | Fido/VIP | AM | Variable | ? | No | Yes | 433 | 2/4 |  |
M |  |  |  |  |  |  |  |  |  |  |  |  |
Motorline |  | AM | Rolling Code | HCS301 | Yes | Yes w/ compatible remote | 433 | 2/4 |  |
Move | ? | AM | Rolling Code | HCS301 | Yes | Yes | 433 | 4 |  |
Mutan | ? | AM | Rolling Code | HCS301? | Yes | Yes w/ compatible remote | 433 | 4 |  |
N |  |  |  |  |  |  |  |  |  |  |  |  |
Nice | Flor | AM | Fixed Code | ? | Yes | Yes w/ compatible remote | 433 | 2/4 |  |
Nice | Smilo | AM | Rolling Code | HCS301? | Yes | Yes w/ compatible remote | 433 | 2 |  |
P |  |  |  |  |  |  |  |  |  |  |  |  |
Prastel | MPSTP MPSTF TRQ 2P TRQ 4P TC2 TC4 | AM | Variable | 42bits | Yes | No | 433 | 2 |  |
Proteco | PTX433 | AM | Fixed | 12bits | Yes | No | 433 | 3 | Similar to TX3 with HT12E and/or eV1527 |
Proteco | TX3 | AM | Fixed | 12bits | Yes | Yes | 433 | 3 | Similar to TX3 with HT12E and/or eV1527 |
Pujol | Vario | AM | Rolling Code? | HCS301? | Yes | Yes | 433 | 3 | Tested on Yellow plastic case remote |
T |  |  |  |  |  |  |  |  |  |  |  |  |
Tango |  | AM | Fixed Code | ? | Yes | Yes w/ compatible remote | 433 | 2/4 |  |
V |  |  |  |  |  |  |  |  |  |  |  |  |
V2 | Phoenix | AM | Variable | 52bits | Yes | Yes | 433 | 4 |  |

Manufacturer | Model | Modulation | Encoding Method | Encoding Type | Compatibility | Verified | Frequency | Buttons | Comments | Front | Back | Inside |
A |  |  |  |  |  |  |  |  |  |  |  |  |
Aprimatic | TR2 TR4 | AM | Rolling Code | HCS301? | Yes | Yes w/ compatible remote | 433 | 2/4 |  |
Avidsen | 104250 | AM | Fixed Code | ? | Yes | Yes w/ compatible remote | 433 | 4 |  |
Avidsen | 104251 | AM | Fixed Code | ? | Yes | Yes | 433 | 4 |  |
Avidsen | 104257 | AM | Fixed Code | ? | Yes | Yes w/ compatible remote | 433 | 4 |  |
Avidsen | 104715 | AM | Fixed Code/ Learning Remote | ? | Yes | Yes | 433 | 4 |  |
B |  |  |  |  |  |  |  |  |  |  |  |  |
Beninca | TO GO T4 WV T4 WK CUPIDO | AM | Rolling Code | HCS301? | Yes | Yes | 433 | 4 |  |
BFT | Mitto | AM | Rolling Code | HCS301 | Yes | Yes | 433 | 2 | Rolling Code emulated in a PIC 12F609 |
C |  |  |  |  |  |  |  |  |  |  |  |  |
Came | TOP432 | AM | Fixed | 12bits | Yes | Yes w/ compatible remote | 433 | 2 | The Came Top432na is two button version of this self-learning remote control series. The four button version Came Top434NA. Came Top432na is made fully compatible with Came 432M, Came 434M, Came 432S, Came 432SA and Came 434MA. Came Top432na is remote control transmitting at 433.92 MHz, the all possible code combinations are as many as 4096 codes. |
Came | TOP434 | AM | Fixed | 12bits | Yes | No | 433 | 4 | The Came Top432na is two button version of this self-learning remote control series. The four button version Came Top434NA. Came Top432na is made fully compatible with Came 432M, Came 434M, Came 432S, Came 432SA and Came 434MA. Came Top432na is remote control transmitting at 433.92 MHz, the all possible code combinations are as many as 4096 codes. |
Cardin | S449 | FM | ? | ? | No | Yes | 433 | 4 |  |
D |  |  |  |  |  |  |  |  |  |  |  |  |
DEA | GENIE MIO TR-2 | AM | Rolling Code | HCS301? | Yes | Yes w/ compatible remote | 433 | 2/4 |  |
Ditec | GOL4 | AM | Variable | 54bits | Yes | Yes w/ compatible remote | 433 | 4 | Ditec GOL4 is a rolling code remote, which has white LED cover color, while GOL4C is a fixed code remote, which has a red LED cover color. |
Ditec | GOL4C | AM | Fixed | 37bits | Yes | Yes | 433 | 4 | Ditec GOL4 is a rolling code remote, which has white LED cover color, while GOL4C is a fixed code remote, which has a red LED cover color. |
Ditec | BILXP2 | AM | Fixed? | 37bits? | Yes | Yes | 433 | 2/4 |  |
Doorhan |  | AM | Rolling Code | HCS301? | Yes | Yes w/ compatible remote | 433 | 4 |  |
E |  |  |  |  |  |  |  |  |  |  |  |  |
Erreka | SOL2R SOL4R ROLLER4 | AM | Rolling Code | HCS301? | Yes | Yes w/ compatible remote | 433 | 4 |  |
Etdoor | ? | AM | ? | ? | Yes | Yes w/ compatible remote | 433 | 2 |  |
F |  |  |  |  |  |  |  |  |  |  |  |  |
FAAC | XT4 433 | AM | Rolling Code | HCS301? | Yes | Yes w/ compatible remote | 433 | 2/4 |  |
Fox |  | AM | Rolling Code | HCS301? | Yes | Yes w/ compatible remote | 433 | 2 |  |
G |  |  |  |  |  |  |  |  |  |  |  |  |
GBD | DOMINO AU1600 | AM | Rolling Code | HCS301? | Yes | Yes w/ compatible remote | 433 | 2 |  |
K |  |  |  |  |  |  |  |  |  |  |  |  |
Key | TXP-42 | AM | Million Code | HT6P20 28bits | Yes | Yes | 433 | 2 |  |
Key | ? | AM | Million Code | eV1527 24bits | Yes | Yes | 433 | 4 |  |
KINGgates | ? | AM | Encrypted |  | Yes | Yes | 433 | 4 |  |
L |  |  |  |  |  |  |  |  |  |  |  |  |
Life | Fido/VIP | AM | Variable | ? | No | Yes | 433 | 2/4 |  |
M |  |  |  |  |  |  |  |  |  |  |  |  |
Motorline |  | AM | Rolling Code | HCS301 | Yes | Yes w/ compatible remote | 433 | 2/4 |  |
Move | ? | AM | Rolling Code | HCS301 | Yes | Yes | 433 | 4 |  |
Mutan | ? | AM | Rolling Code | HCS301? | Yes | Yes w/ compatible remote | 433 | 4 |  |
N |  |  |  |  |  |  |  |  |  |  |  |  |
Nice | Flor | AM | Fixed Code | ? | Yes | Yes w/ compatible remote | 433 | 2/4 |  |
Nice | Smilo | AM | Rolling Code | HCS301? | Yes | Yes w/ compatible remote | 433 | 2 |  |
P |  |  |  |  |  |  |  |  |  |  |  |  |
Prastel | MPSTP MPSTF TRQ 2P TRQ 4P TC2 TC4 | AM | Variable | 42bits | Yes | No | 433 | 2 |  |
Proteco | PTX433 | AM | Fixed | 12bits | Yes | No | 433 | 3 | Similar to TX3 with HT12E and/or eV1527 |
Proteco | TX3 | AM | Fixed | 12bits | Yes | Yes | 433 | 3 | Similar to TX3 with HT12E and/or eV1527 |
Pujol | Vario | AM | Rolling Code? | HCS301? | Yes | Yes | 433 | 3 | Tested on Yellow plastic case remote |
R |  |  |  |  |  |  |  |  |  |  |  |  |
Roger | TX12 | AM | Fixed Code | 27bits | Yes | Yes w/ compatible remote | 433 | 2/4 |  |
Roger | TX14 | AM | Fixed Code | 27bits | Yes | Yes w/ compatible remote | 433 | 2/4 |  |
Roger | TX22 | AM | Fixed Code | 27bits | Yes | Yes w/ compatible remote | 433 | 2/4 |  |
T |  |  |  |  |  |  |  |  |  |  |  |  |
Tango |  | AM | Fixed Code | ? | Yes | Yes w/ compatible remote | 433 | 2/4 |  |
V |  |  |  |  |  |  |  |  |  |  |  |  |
V2 | Phoenix | AM | Variable | 52bits | Yes | Yes | 433 | 4 |  |
Notes: | (1) Rolling Code Security measurements implementated only in LMPAutomation Remotes. |  |  |  |  |  |  |